|  |  |  |  |
| --- | --- | --- | --- |
| **MCCB 3P - Chỉnh dòng nhiệt (Adj. thermal)**  **30 ~ 250AF (0.8-0.9-1\*In), 400 ~ 800AF (0.63-0.8-1\*In)** | | | |
| HGM50E-F 3P | 16-20-25-32-40-50A | 16kA | 650,000 |
| HGM50S-F 3P | 16-20-25-32-40-50A | 20kA | 670,000 |
| HGM50H-F 3P | 16-20-25-32-40-50A | 38kA | 790,000 |
| HGM100E-F 3P | 63-75-100A | 16kA | 850,000 |
| HGM100H-F 3P | 63-75-100A | 26kA | 920,000 |
| HGM100L-F 3P | 63-75-100A | 30kA | 950,000 |
| HGM125E-F 3P | 75-100-125A | 20kA | 880,000 |
| HGM125S-F 3P | 75-100-125A | 26kA | 920,000 |
| HGM125H-F 3P | 75-100-125A | 38kA | 1,150,000 |
| HGM250S-F 3P | 100~250A | 26kA | 1,650,000 |
| HGM250H-F 3P | 100~250A | 38kA | 1,850,000 |
| HGM250L-F 3P | 125~250A | 55kA | 2,150,000 |
| HGM400E-F 3P | 250-300-350-400A | 45kA | 4,150,000 |
| HGM400S-F 3P | 250-300-350-400A | 65kA | 4,550,000 |
| HGM400H-F 3P | 250-300-350-400A | 85kA | 4,650,000 |
| HGM630E-F 3P | 500-630A | 45kA | 8,300,000 |
| HGM630S-F 3P | 500-630A | 65kA | 9,500,000 |
| HGM630H-F 3P | 500-630A | 85kA | 9,600,000 |
| HGM800S-F 3P | 700-800A | 65kA | 9,600,000 |
| HGM800H-F 3P | 700-800A | 85kA | 10,200,000 |

# | High performance



**\* Ui: 1,000V**

* **Uimp: 8kV**
* **Ics = 100% Icu**

**| Approvals and Certification**



|  |  |  |  |
| --- | --- | --- | --- |
| **Mã hàng** | **In(A)** | **Icu(kA)** | **Đơn giá(VND)** |
| **MCCB 2P - Chỉnh dòng nhiệt (Adj. thermal)**  **30 ~ 250AF (0.8-0.9-1\*In), 400 ~ 800AF (0.63-0.8-1\*In)** | | | |
| HGM50E-F 2P | 16-20-25-32-40-50A | 35kA | 550,000 |
| HGM100E-F 2P | 63-75-100A | 35kA | 680,000 |
| HGM125E-F 2P | 75-100-125A | 50kA | 830,000 |
| HGM250E-F 2P | 125~250A | 50kA | 1,380,000 |
| HGM400E-F 2P | 250/300/350/400A | 50kA | 3,400,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Mã hàng** | **In(A)** | **Icu(kA)** | **Đơn giá(VND)** |
| **MCCB 4P - Chỉnh dòng nhiệt (Adj. thermal)**  **30 ~ 250AF (0.8-0.9-1\*In), 400 ~ 800AF (0.63-0.8-1\*In)** | | | |
| HGM60E-F 4P | 16~63A | 16kA | 1,050,000 |
| HGM60S-F 4P | 16~63A | 20kA | 1,250,000 |
| HGM60H-F 4P | 16~63A | 26kA | 1,350,000 |
| HGM60L-F 4P | 16~63A | 30kA | 1,450,000 |
| HMG100S-F 4P | 75-100A | 20kA | 1,350,000 |
| HMG100H-F 4P | 75-100A | 26kA | 1,400,000 |
| HMG100L-F 4P | 75-100A | 30kA | 1,500,000 |
| HMG125E-F 4P | 100-125A | 20kA | 1,850,000 |
| HMG125H-F 4P | 100-125A | 38kA | 1,900,000 |
| HMG250E-F 4P | 125~250A | 20kA | 2,750,000 |
| HMG250S-F 4P | 125~250A | 26kA | 2,850,000 |
| HMG250H-F 4P | 125~250A | 38kA | 3,050,000 |
| HMG400E-F 4P | 250-300-350-400A | 45kA | 5,800,000 |
| HMG400S-F 4P | 250-300-350-400A | 65kA | 6,000,000 |
| HMG400H-F 4P | 250-300-350-400A | 85kA | 6,200,000 |
| HMG630E-F 4P | 500-630A | 45kA | 10,500,000 |
| HMG630S-F 4P | 500-630A | 65kA | 11,000,000 |
| HMG630H-F 4P | 500-630A | 85kA | 12,000,000 |
| HMG800S-F 4P | 700-800A | 65kA | 12,000,000 |
| HMG800H-F 4P | 700-800A | 85kA | 12,500,000 |

(\*) AC200~230V, AC380~415V

|  |  |  |
| --- | --- | --- |
| **Phụ kiện MCCB** | | |
| Aux. Switch | AUX 10GM C1 (HMG30~250) | 250,000 |
| AUX 40GM (HMG400/ 800) | 350,000 |
| Alarm Switch | ALT 10GM (HMG30~250) | 250,000 |
| ALT 40GM (HGM400/ 800) | 350,000 |
| Shunt Trip (\*) | SHT 10GM (HMG30~250) | 450,000 |
| SHT 40GM (HMG400/ 800) | 690,000 |
| Under Voltage Trip (\*) | UVT 10GM (HGM30~250) | 1,200,000 |
| UVT 40GM (HGM400/ 800) | 1,200,000 |
| Tay xoay (Handle) | TFG/ TFH | (\*\*) |
| Motor (MOT) | MOT | (\*\*) |
| Nắp đầu cực | TCF | (\*\*) |
| Tấm chắn pha | TQQ | (\*\*) |
| Khoá (Padlock) | PLD | (\*\*) |
| Thanh cái (Bus bar) | TBB 40GM 3S cho HMG400 3P | 990,000 |
|  | TBB 80GM 3S cho HMG630/800 3P | 1,800,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **MCCB 3P -**  **Chỉnh dòng nhiệt (0.8-1\*In) và dòng INST (5-10\*In)** | | | |
| HGP400S-H 3P | 250-300-350-400A | 65kA | 6,600,000 |
| HGP630S-H 3P | 500-630A | 65kA | 12,500,000 |
| HGP800S-H 3P | 700-800A | 65kA | 14,200,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **MCCB 3P - Chỉnh dòng điện tử (Electronic)** | | | |
| UPB400S 3P | 200~400A | 85kA | 12,000,000 |
| UPB400H 3P | 200~400A | 100kA | 12,500,000 |
| UPB630S 3P | 320~630A | 85kA | 13,500,000 |
| UPB630H 3P | 320~630A | 100kA | 14,000,000 |

(\*\*) Quý khách vui lòng liên hệ Nhà phân phối

|  |  |  |  |
| --- | --- | --- | --- |
| **Mã hàng** | **In(A)** | **Icu (kA)** | **Đơn giá(VNĐ)** |
| **APTOMAT- MCB (Loại thanh cài)** | | | |
| HiBD63-N (1P) | 6~63A | 6 | 61,000 |
| HiBD63-N (2P) | 6~63A | 6 | 135,000 |
| HiBD63-N (3P) | 6~63A | 6 | 220,000 |
| HiBD63-N (4P) | 6~63A | 6 | 360,000 |
| HiBD63-N (1P+N) | 6~63A | 6 | 135,000 |
| HiBD63-N (3P+N) | 6~63A | 6 | 360,000 |
| HiBD63h (1P) | 6~63A | 10 | 90,000 |
| HiBD63h (2P) | 6~63A | 10 | 200,000 |
| HiBD63h (3P) | 6~63A | 10 | 330,000 |
| HiBD125 (1P) | 63~125A | 10 | 165,000 |
| HiBD125 (2P) | 63~125A | 10 | 365,000 |
| HiBD125 (3P) | 63~125A | 10 | 595,000 |
| HiBD125 (4P) | 63~125A | 10 | 990,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Mã hàng** | **In(A)** | **Icu (kA)** | **Đơn giá(VNĐ)** |
| **APTOMAT RCBO (dòng dò 10/ 30/ 100/ 300/ 500mA)** | | | |
| HiRO40 (1P+N) | 10-16-20-25-32-40A | 4.5 | 498,000 |
| **APTOMAT RCCB (dòng dò 10/ 30/ 100/ 300/ 500mA)** | | | |
| HiRC63 2PG | 16 -25 -32 -40 -63A | | 520,000 |
| HiRC63 4PG | 16 -25 -32 -40 -63A | | 620,000 |

|  |  |  |
| --- | --- | --- |
| **SWITCH DISCONNECTOR** | | |
| HiSD125 1P | 16 - 32 - 63A | 60,000 |
| 100 - 125A | 95,000 |
| HiSD125 2P | 16 - 32 - 63A | 120,000 |
| 100 - 125A | 190,000 |
| HiSD125 3P | 16 - 32 - 63A | 190,000 |
| 100 - 125A | 300,000 |
| HiSD125 4P | 16 - 32 - 63A | 250,000 |
| 100 - 125A | 395,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **APTOMAT- MCCB 2P (Loại hộp đúc)** | | | |
| HiBC32S (ko vỏ) | 10-15-20-30A | 1.5 | (\*\*) |
| UDB30S 2P | 10-15-20-30A | 5 | 375,000 |
| UDB50S 2P | 40-50A | 5 | 420,000 |
| UAB50R 2P | 40-50A | 25 | 575,000 |
| UAB60R 2P | 60A | 25 | 630,000 |
| UAB100C 2P | 75-100A | 25 | 650,000 |
| UCB250R 2P | 125~250A | 35 | 1,800,000 |
| UCB400R 2P | 250-300-350-400A | 35 | 3,750,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **APTOMAT- MCCB 3P, Chỉnh dòng Electronic** | | | |
| UPB400S 3P | 200~400A | 85 | 12,000,000 |
| UPB400H 3P | 200~400A | 100 | 12,500,000 |
| UPB630S 3P | 320~630A | 85 | 13,500,000 |
| UPB630H 3P | 320~630A | 100 | 14,000,000 |
| UCB1000S 3P | 505~1000A | 100 | 22,500,000 |
| UCB1250S 3P | 630~1250A | 100 | 24,500,000 |
| UCB1600S 3P | 640~1600A | 65 | 48,500,000 |

## 

|  |  |  |  |
| --- | --- | --- | --- |
| **APTOMAT- MCCB 3P (Loại hộp đúc)** | | | |
| UDB30S 3P | 10-15-20-30A | 2.5 | 505,000 |
| UDB50S 3P | 40-50A | 2.5 | 520,000 |
| UAB30C 3P | 10-15-20-30A | 7.5/5 | 730,000 |
| UAB30R 3P | 10-15-20-30A | 14/10 | 750,000 |
| UAB50R 3P | 40-50A | 14/10 | 750,000 |
| UAB60R 3P | 60A | 14/10 | 790,000 |
| UAB100C 3P | 75-100A | 14/10 | 820,000 |
| UAB100R 3P | 75-100A | 25 | 900,000 |
| UCB50R 3P | 40-50A | 30/25 | 1,050,000 |
| UCB100R 3P | 75-100-125A | 30/25 | 1,250,000 |
| UCB100S 3P | 75-100-125A | 42/36 | 1,350,000 |
| UCB250S 3P | 125~250A | 35/25 | 1,950,000 |
| UCB250H 3P | 125~250A | 42 | 2,000,000 |
| UCB400R 3P | 250-300-350-400A | 30 | 4,080,000 |
| UCB400S 3P | 250-300-350-400A | 42 | 4,250,000 |
| UCB400H 3P | 250-300-350-400A | 65 | 4,400,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **APTOMAT- MCCB 4P (Loại hộp đúc)** | | | |
| UAB50R 4P | 10-15-20-30-40-50A | 7.5/5 | 950,000 |
| UAB60R 4P | 60A | 7.5/5 | 980,000 |
| UAB100C 4P | 75-100A | 14/10 | 1,010,000 |
| UCB100R 4P | 75-100A | 30/25 | 1,750,000 |
| UCB250R 4P | 125~250A | 25/18 | 2,560,000 |
| UCB400R 4P | 250-300-350-400A | 30 | 5,500,000 |
| UCB630R-F 4P | 500-630A | 45 | 10,400,000 |
| UCB800R-F 4P | 700-800A | 45 | 11,000,000 |
| UCB1000S 4P | 505~1000A | 100 | 29,000,000 |
| UCB1250S 4P | 630~1250A | 100 | 33,500,000 |

(\*\*) Quý khách vui lòng liên hệ Nhà phân phối

|  |  |  |
| --- | --- | --- |
| **PHỤ KIỆN MCCB** | | |
| Tiếp điểm  (AUX hoặc ALT) | UAB30C~100C, UAB30R~60R | 250,000 |
| UCB250R/S/N | 250,000 |
| UCB400~800 | 375,000 |
| UCB1000~1250S/L | 720,000 |
| Shunt Trip (SHT) | SHT 10A\_ | 450,000 |
| SHT 20C\_ | 450,000 |
| SHT 46D\_ | 690,000 |
| SHT 120NE\_ | 1,500,000 |
| Under Voltage Trip (UVT) | UVT 10A\_ | 1,200,000 |
| UVT 20C\_ | 1,200,000 |
| UVT 46D\_ | 750,000 |
| UVT 120NE\_ | 750,000 |
| BUS BAR | TBB4S 3 (UCB400R/S/H/L) | 1,080,000 |
| TBB6S 3 (UCB630R/S/H/L) | 1,800,000 |
| TBB8S 3 (UCB800R/S/H/L) | 2,100,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **APTOMAT- MCCB 3P, Chỉnh dòng nhiệt (0.8~1)In** | | | |
| UCB250S-F 3P | 125~250A | 35/25 | 2,100,000 |
| UCB400S-F 3P | 250-300-350-400 | 42 | 4,550,000 |
| UCB400H-F 3P | 250-300-350-400 | 65 | 4,600,000 |
| UCB630R-F 3P | 500-630A | 45 | 8,300,000 |
| UCB630S-F 3P | 500-630A | 65 | 9,500,000 |
| UCB630H-F 3P | 500-630A | 85 | 9,600,000 |
| UCB800R-F 3P | 700-800A | 45 | 8,750,000 |
| UCB800S-F 3P | 700-800A | 65 | 9,980,000 |
| UCB800H-F 3P | 700-800A | 85 | 10,080,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Mã hàng** | **In(A)** | **Công suất** | **Đơn giá (VNĐ)** |
| **CONTACTOR 3 PHA (AC Magnetic Contactor, 380VAC, 50Hz)** | | | |
| HGC9 11NS X --- | 9A (1a1b) | 4KW | 268,000 |
| HGC12 11NS X --- | 12A(1a1b) | 5.5KW | 290,000 |
| HGC18 11NS X --- | 18A(1a1b) | 7.5KW | 390,000 |
| HGC25 11NS X --- | 25A(1a1b) | 11KW | 475,000 |
| HGC32 22NS X --- | 32A(2a2b) | 15KW | 690,000 |
| HGC40 22NS X --- | 40A(2a2b) | 18.5KW | 830,000 |
| HGC50 22NS X --- | 50A(2a2b) | 22KW | 915,000 |
| HGC65 22NS X --- | 65A(2a2b) | 30KW | 1,150,000 |
| HGC75 22NS X --- | 75A(2a2b) | 37KW | 1,450,000 |
| HGC85 22NS X --- | 85A(2a2b) | 45KW | 1,750,000 |
| HGC100 22NS X --- | 100A(2a2b) | 55KW | 2,150,000 |
| **CONTACTOR 3 PHA (AC/DC Magnetic Contactor)** | | | |
| HGC115 22NS F --- | 115A(2a2b) | 60KW | 2,640,000 |
| HGC130 22NS F --- | 130A(2a2b) | 65KW | 2,750,000 |
| HGC150 22NS F --- | 150A(2a2b) | 75KW | 3,500,000 |
| HGC185 22NS F --- | 185A(2a2b) | 90KW | 4,600,000 |
| HGC225 22NS F --- | 225A(2a2b) | 132KW | 5,300,000 |
| HGC265 22NS F --- | 265A(2a2b) | 147KW | 7,150,000 |
| HGC300 22NS F --- | 300A(2a2b) | 160KW | 7,800,000 |
| HGC400 22NS F --- | 400A(2a2b) | 220KW | 9,000,000 |
| HGC500 22NS F --- | 500A(2a2b) | 250KW | 15,500,000 |
| HGC630 22NS F --- | 630A(2a2b) | 330KW | 18,900,000 |
| HGC800 22NS F --- | 800A(2a2b) | 400KW | 24,000,000 |

|  |  |  |
| --- | --- | --- |
| **Mã hàng** | **Tiếp điểm** | **Đơn giá (VNĐ)** |
| **TIẾP ĐIỂM PHỤ (CÀI TRÊN)** | | |
| HCBTB--NS  cho HGC9-HGC100 | 2NC/ 1NO+1NC/ 2NC | 85,000 |
| 4NO/3NO+1NC  2NO+2NC/  1NO+3NC/4NC | 150,000 |

|  |  |  |
| --- | --- | --- |
| **TIẾP ĐIỂM PHỤ (CÀI CẠNH)** | | |
| HGCSB 40 | 1NO+1NC, cho HGC9-HGC40 | 85,000 |
| HGCSB 100 | 1NO+1NC,  cho HGC50-HGC100 | 120,000 |
| HGCSB 800 | 1NO+1NC,  cho HGC115-HGC800 | 160,000 |

|  |  |  |
| --- | --- | --- |
| **KHÓA LIÊN ĐỘNG** | | |
| HGCIU40 | HGC9 ~ HGC40 | 150,000 |
| HGCIU100 | HGC50 ~ HGC100 | 180,000 |
| HGCIU265 | HGC115 ~ HGC265 | 250,000 |
| HGCIU800 | HGC300 ~ HGC800 | 1,200,000 |

|  |  |  |
| --- | --- | --- |
| **CONTROL RELAY (4b/ 1a3b/ 2a2b/ 3a1b/ 4a)** | | |
| HGR--XS X220 | AC220V | 430,000 |
| HGR--TS D110 | DC110V | 540,000 |

|  |  |  |
| --- | --- | --- |
| **CUỘN HÚT CONTACTOR (AC, AC/DC Coil)** | | |
| HGCOL18 X--- | cho HGC9-HGC18 | 138,000 |
| HGCOL40 X--- | cho HGC25-HGC40 | 138,000 |
| HGCOL65 X--- | cho HGC50-HGC65 | 196,000 |
| HGCOL100 X--- | cho HGC75-HGC100 | 220,000 |
| HGCOL150 F--- | cho HGC115-HGC150 | 1,150,000 |
| HGCOL265 F--- | cho HGC185-HGC265 | 1,480,000 |
| HGCOL500 F--- | cho HGC300-HGC500 | 2,620,000 |
| HGCOL800 F-- | cho HGC630-HGC800 | 3,520,000 |

|  |  |  |
| --- | --- | --- |
| **RƠ LE NHIỆT** | **Dải dòng** | **Đơn giá (VNĐ)** |
|  | 0.12 - 0.18A, 0.18 - 0.26A, |  |
|  | 0.25 - 0.35A, 0.34 - 0.5A, |  |
| HGT18K  (cho HGC9 ~ HGC18) | 0.5 - 0.7A, 0.6 - 0.9A,  0.8 - 1.2A, 1.1 - 1.6A,  1.5 - 2.1A, 2 - 3A,  2.8 - 4.2A, 3 - 5A, | 230,000 |
|  | 4 - 6A, 5.6 - 8A, |  |
|  | 6 - 9A, 8 - 12A, 12 - 18A |  |
| HGT40K  (cho HGC25~HGC40) | 8 - 12A, 12 - 18A,15 - 22A,  17 - 25A, 22 - 32A, 28-40A | 280,000 |
| HGT65K  (cho HGC50~HGC65) | 17 - 25A, 22-32A, 28 - 40A,  34 - 50A, 45 - 65A | 580,000 |
| HGT100K  (cho HGC75~HGC100 ) | 28 - 40A,34 - 50A, 45 - 65A,  52 - 75A, 59 - 85A, 70-100A | 845,000 |
| HGT150K  (cho HGC115~HGC150) | 48 - 80A, 69 - 115A,  78 - 130A, 90 - 150A | 1,650,000 |
| HGT265K  (cho HGC185~HGC265) | 90 - 150A, 111 - 185A,  135 - 225A, 159 - 265A | 2,150,000 |
| HGT500K  (cho HGC300~HGC500) | 159 - 265A,180 - 300A,  240 - 400A, 300-500A | 3,000,000 |
| UTH800K  (cho HGC630, HGM800) | 378 - 630A, 480 - 800A | 6,000,000 |

|  |  |  |
| --- | --- | --- |
| **CUỘN HÚT CONTACTOR (DC Coil)** | | |
| HGCOL18 D--- | cho HGC9-HGC18 | 210,000 |
| HGCOL40 D--- | cho HGC25-HGC40 | 220,000 |
| HGCOL65 D--- | cho HGC50-HGC65 | 230,000 |
| HGCOL100 D--- | cho HGC75-HGC100 | 260,000 |

|  |  |  |
| --- | --- | --- |
| **CONTACTOR 3 PHA (DC COIL)** | | |
| HGC9 11NSD--- | 9A (1a1b) | 450,000 |
| HGC12 11NSD--- | 12A(1a1b) | 475,000 |
| HGC18 11NSD--- | 18A(1a1b) | 560,000 |
| HGC25 11NSD--- | 25A(1a1b) | 575,000 |
| HGC32 11NSD--- | 32A (1a1b) | 750,000 |
| HGC40 11NSD--- | 40A (1a1b) | 950,000 |
| HGC50 11NSD--- | 50A (1a1b) | 1,050,000 |
| HGC65 11NSD--- | 65A (1a1b) | 1,350,000 |
| HGC75 11NSD--- | 75A (1a1b) | 1,950,000 |
| HGC85 11NSD--- | 85A (1a1b) | 2,400,000 |
| HGC100 11NSD--- | 100A (1a1b) | 2,500,000 |

|  |  |  |
| --- | --- | --- |
| **CAPACITOR SWITCHING UNIT**  **(Phụ kiện Contactor khi sử dụng cho đóng cắt tụ bù)** | | |
| HGCCU40 10N (1NO) | cho HGC9-HGC40 | 390,000 |
| HGCCU40 01N (1NC) | 390,000 |
| HGCCU100 10N (1NO) | cho HGC50-HGC100 | 405,000 |
| HGCCU100 01N (1NC) | 405,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Mã hàng** | **In(A)** | **Công suất** | **Đơn giá(VNĐ)** |
| **CONTACTOR 3 PHA (AC Magnetic Contactor, 380VAC, 50Hz)** | | | |
| UMC9 11NS X --- | 9A (1a1b) | 4KW | 265,000 |
| UMC12 11NS X --- | 12A(1a1b) | 5.5KW | 290,000 |
| UMC18 11NS X --- | 18A(1a1b) | 7.5KW | 380,000 |
| UMC25 11NS X --- | 25A(1a1b) | 11KW | 450,000 |
| UMC32 22NS X --- | 32A(2a2b) | 15KW | 650,000 |
| UMC40 22NS X --- | 40A(2a2b) | 18.5KW | 780,000 |
| UMC50 22NS X --- | 50A(2a2b) | 22KW | 880,000 |
| UMC65 22NS X --- | 65A(2a2b) | 30KW | 1,100,000 |
| UMC75 22NS X --- | 75A(2a2b) | 37KW | 1,500,000 |
| UMC85 22NS X --- | 85A(2a2b) | 45KW | 1,750,000 |
| UMC100 22NS X --- | 100A(2a2b) | 55KW | 2,050,000 |
| **CONTACTOR 3 PHA (AC/DC Magnetic Contactor)** | | | |
| UMC115 22NS F --- | 115A(2a2b) | 60KW | 2,200,000 |
| UMC130 22NS F --- | 130A(2a2b) | 65KW | 2,750,000 |
| UMC150 22NS F --- | 150A(2a2b) | 75KW | 3,200,000 |
| UMC185 22NS F --- | 185A(2a2b) | 90KW | 4,400,000 |
| UMC225 22NS F --- | 225A(2a2b) | 132KW | 5,100,000 |
| UMC265 22NS F --- | 265A(2a2b) | 147KW | 6,600,000 |
| UMC300 22NS F --- | 300A(2a2b) | 160KW | 7,300,000 |
| UMC400 22NS F --- | 400A(2a2b) | 220KW | 10,500,000 |
| UMC500 22NS F --- | 500A(2a2b) | 250KW | 14,500,000 |
| UMC630 22NS F --- | 630A(2a2b) | 330KW | 17,500,000 |
| UMC800 22NS F --- | 800A(2a2b) | 400KW | 22,500,000 |

|  |  |  |
| --- | --- | --- |
| **Mã hàng** | **Tiếp điểm** | **Đơn giá (VNĐ)** |
| **TIẾP ĐIỂM PHỤ** | | |
| UAB 02NS | 2NC/ 1NO+1NC/ 2NO  Cài trên, cho UMC9- UMC100, UMX, & UMT | 85,000 |
| UAB 11NS |
| UAB 20NS |
| UAB 04NS | 4NO, 4NC, 1NO+3NC,  2NO+2NC, 3NO+1NC,  (Cài trên, cho UMC9- UMC100, UMX, & UMT) | 150,000 |
| UAB 13NS |
| UAB 22NS |
| UAB 31NS |
| UAB 40NS |
| UAL65 11NS | 1NO+1NC, Cài bên, cho UMC9-UMC65 | 85,000 |
| UAL100 11NS | 1NO+1NC, Cài bên, cho UMC75-UMC100 | 120,000 |
| UAL400 11NS | 1NO+1NC, Cài bên, cho UMC115-UMC800 | 140,000 |
| **KHÓA LIÊN ĐỘNG** | | |
| UTL65 | UMC9 ~ UMC65 | 150,000 |
| UTL100 | UMC75 ~ UMC100 | 180,000 |
| UTL265 | UMC115 ~ UMC265 | 250,000 |
| UTL400 | UMC300 ~ UMC800 | 900,000 |

|  |  |  |
| --- | --- | --- |
| **CONTROL RELAY (4b/ 1a3b/ 2a2b/ 3a1b/ 4a)** | | |
| UMX--NS X220 | AC220V | 430,000 |
| UMT--NS D110 | DC110V | 580,000 |

|  |  |  |
| --- | --- | --- |
| **RƠ LE NHIỆT** | **Dải dòng** | **Đơn giá (VNĐ)** |
|  | 0.12 - 0.18A, 0.18 - 0.26A, |  |
|  | 0.25 - 0.35A, 0.34 - 0.5A, |  |
|  | 0.5 - 0.7A, 0.6 - 0.9A, |  |
| UTH12H (2 Elements,  cho UMC9 & UMC12) | 0.8 - 1.2A, 1.1 - 1.6A,  1.5 - 2.1A, 2 - 3A, | 220,000 |
|  | 2.8 - 4.2A, 3 - 5A, |  |
|  | 4 - 6A, 5.6 - 8A, |  |
|  | 6 - 9A, 8 - 12A |  |
| UTH32H (2 Elements, cho UMC18~UMC32) | 6 - 9A, 8 - 12A, 12 - 18A,  15 - 22A, 17 - 25A,  22 - 32A | 280,000 |
|  | 7A - 10A, 8 - 12A, |  |
| UTH65H (2 Elements,  cho UMC40~UMC65) | 12 - 18A,15 - 22A,  17 - 25A, 28 - 40A, 34 - 50A, | 480,000 |
|  | 45 - 65A |  |
| UTH100H (2 Elements, cho UMC75~UMC100 ) | 34 - 50A, 45 - 65A,  52 - 75A, 59 - 85A, 70-100A | 600,000 |
| UTH150K (3 Element, cho UMC115~UMC150) | 48 - 80A, 69 - 115A,  78 - 130A, 90 - 150A | 1,650,000 |
| UTH265K (3 Element, cho UMC185~UMC265) | 90 - 150A, 111 - 185A,  135 - 225A, 159 - 265A | 2,150,000 |
| UTH400K (3 Element,  cho UMC300, 400) | 135 - 225A, 159 - 265A,  180 - 300A, 240 - 400A | 3,050,000 |
| UTH800K (3 element, cho UMC500) | 300 - 500A | 3,500,000 |
| UTH800K (3 element,  cho UMC630, 800) | 378 - 630A, 480 - 800A | 6,000,000 |

|  |  |  |
| --- | --- | --- |
| **CUỘN HÚT CONTACTOR (AC, AC/DC Coil)** | | |
| UMCOL12 X--- | cho UMC9-UMC12, UMX | 90,000 |
| UMCOL32 X--- | cho UMC18-UMC32 | 90,000 |
| UMCOL65 X--- | cho UMC40-UMC65 | 140,000 |
| UMCOL100 X--- | cho UMC75-UMC100 | 200,000 |
| UMCOL150 F--- | cho UMC115-UMC150 | 900,000 |
| UMCOL265 F--- | cho UMC185-UMC265 | 1,500,000 |
| UMCOL400 F--- | cho UMC300-UMC500 | 2,000,000 |

|  |  |  |
| --- | --- | --- |
| **Thiết bị chống sốc điện (Surge Absorber)** | | |
| URC32 Y --- (UMC9~UMC32) | AC24V-48V, AC110V- 220V, AC240V-380V | 150,000 |
| URC100 Y --- (UMC40~UMC100) | AC24V-48V, AC110V- 220V, AC240V-380V | 150,000 |

|  |  |  |
| --- | --- | --- |
| **Capacitor Switching Unit** | | |
| UAD100 10NS | 1 NO | 400,000 |
| UAD100 01NS | 1 NC | 400,000 |

## 

|  |  |  |  |
| --- | --- | --- | --- |
| **Mã hàng** | **In (A)** | **Icu(kA)** | **Đơn giá(VND)** |
| **MÁY CẮT KHÔNG KHÍ - ACB 3P UAS type, loại cố định** | | | |
| UAS06A 3H M2C2S250T | 630A | 65 | 42,000,000 |
| UAS08A 3H M2C2S250H | 800A | 65 | 42,500,000 |
| UAS10A 3H M2C2S250J | 1000A | 65 | 44,000,000 |
| UAS12A 3H M2C2S250K | 1250A | 65 | 46,000,000 |
| UAS16A 3H M2C2S250L | 1600A | 65 | 48,000,000 |
| UAS20B 3H M2C2S250M | 2000A | 85 | 60,000,000 |
| UAS25B 3H M2C2S250N | 2500A | 85 | 66,000,000 |
| UAS32B 3H M2C2S250P | 3200A | 85 | 76,500,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Mã hàng** | **In (A)** | **Icu(kA)** | **Đơn giá(VND)** |
| **MÁY CẮT KHÔNG KHÍ - ACB 3P UAS type, loại ngăn kéo** | | | |
| UAS06A 3B M2C2S250T | 630A | 65 | 56,500,000 |
| UAS08A 3B M2C2S250H | 800A | 65 | 58,000,000 |
| UAS10A 3B M2C2S250J | 1000A | 65 | 59,000,000 |
| UAS12A 3B M2C2S250K | 1250A | 65 | 63,500,000 |
| UAS16A 3B M2C2S250L | 1600A | 65 | 66,000,000 |
| UAS20B 3B M2C2S250M | 2000A | 85 | 78,000,000 |
| UAS25B 3B M2C2S250N | 2500A | 85 | 86,000,000 |
| UAS32B 3B M2C2S250P | 3200A | 85 | 96,000,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **MÁY CẮT KHÔNG KHÍ - ACB 3P UAN type, loại cố định** | | | |
| UAN06A 3H M2C2S250T | 630A | 85 | 45,500,000 |
| UAN08A 3H M2C2S250H | 800A | 85 | 47,000,000 |
| UAN10A 3H M2C2S250J | 1000A | 85 | 48,000,000 |
| UAN12A 3H M2C2S250K | 1250A | 85 | 50,000,000 |
| UAN16A 3H M2C2S250L | 1600A | 85 | 52,000,000 |
| UAN20A 3V M2C2S250M | 2000A | 85 | 56,000,000 |
| UAN20B 3H M2C2S250M | 2000A | 100 | 65,000,000 |
| UAN25B 3H M2C2S250N | 2500A | 100 | 74,000,000 |
| UAN32B 3H M2C2S250P | 3200A | 100 | 95,000,000 |
| UAN40B 3H M2C2S250Q | 4000A | 100 | 101,000,000 |
| UAN40C 3H M2C2S250Q | 4000A | 100 | 130,000,000 |
| UAN50C 3H M2C2S250S | 5000A | 100 | 144,000,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **MÁY CẮT KHÔNG KHÍ - ACB 3P UAN type, loại ngăn kéo** | | | |
| UAN06A 3B M2C2S250T | 630A | 85 | 63,000,000 |
| UAN08A 3B M2C2S250H | 800A | 85 | 64,000,000 |
| UAN10A 3B M2C2S250J | 1000A | 85 | 66,000,000 |
| UAN12A 3B M2C2S250K | 1250A | 85 | 71,000,000 |
| UAN16A 3B M2C2S250L | 1600A | 85 | 74,000,000 |
| UAN20A 3B M2C2S250M | 2000A | 85 | 79,000,000 |
| UAN20B 3B M2C2S250M | 2000A | 100 | 89,000,000 |
| UAN25B 3B M2C2S250N | 2500A | 100 | 96,800,000 |
| UAN32B 3B M2C2S250P | 3200A | 100 | 129,000,000 |
| UAN40B 3B M2C2S250Q | 4000A | 100 | 131,000,000 |
| UAN40C 4B M2C2S250Q | 4000A | 100 | 160,000,000 |
| UAN50C 3B M2C2S250S | 5000A | 100 | 168,000,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **MÁY CẮT KHÔNG KHÍ -ACB 4P UAS type, loại cố định** | | | |
| UAS06A 4H M2C2S250T | 630A | 65 | 49,000,000 |
| UAS08A 4H M2C2S250H | 800A | 65 | 49,500,000 |
| UAS10A 4H M2C2S250J | 1000A | 65 | 50,000,000 |
| UAS12A 4H M2C2S250K | 1250A | 65 | 53,000,000 |
| UAS16A 4H M2C2S250L | 1600A | 65 | 54,000,000 |
| UAS20B 4H M2C2S250M | 2000A | 85 | 68,000,000 |
| UAS25B 4H M2C2S250N | 2500A | 85 | 72,000,000 |
| UAS32B 4H M2C2S250P | 3200A | 85 | 81,000,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **MÁY CẮT KHÔNG KHÍ - ACB 4P UAS type, loại ngăn kéo** | | | |
| UAS06A 4B M2C2S250T | 630A | 65 | 68,000,000 |
| UAS08A 4B M2C2S250H | 800A | 65 | 69,500,000 |
| UAS10A 4B M2C2S250J | 1000A | 65 | 70,500,000 |
| UAS12A 4B M2C2S250K | 1250A | 65 | 76,000,000 |
| UAS16A 4B M2C2S250L | 1600A | 65 | 78,500,000 |
| UAS20B 4B M2C2S250M | 2000A | 85 | 93,000,000 |
| UAS25B 4B M2C2S250N | 2500A | 85 | 99,000,000 |
| UAS32B 4B M2C2S250P | 3200A | 85 | 108,000,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **MÁY CẮT KHÔNG KHÍ - ACB 4P UAN type, loại cố định** | | | |
| UAN06A 4H M2C2S250T | 630A | 85 | 54,000,000 |
| UAN08A 4H M2C2S250H | 800A | 85 | 54,500,000 |
| UAN10A 4H M2C2S250J | 1000A | 85 | 55,000,000 |
| UAN12A 4H M2C2S250K | 1250A | 85 | 58,000,000 |
| UAN16A 4H M2C2S250L | 1600A | 85 | 60,000,000 |
| UAN20A 4V M2C2S250M | 2000A | 85 | 65,000,000 |
| UAN20B 4H M2C2S250M | 2000A | 100 | 77,000,000 |
| UAN25B 4H M2C2S250N | 2500A | 100 | 90,000,000 |
| UAN32B 4H M2C2S250P | 3200A | 100 | 112,000,000 |
| UAN40C 4H M2C2S250Q | 4000A | 100 | 165,000,000 |
| UAN50C 4H M2C2S250S | 5000A | 100 | 188,000,000 |

|  |  |  |  |
| --- | --- | --- | --- |
| **MÁY CẮT KHÔNG KHÍ - ACB 4P UAN type, loại ngăn kéo** | | | |
| UAN06A 4B M2C2S250T | 630A | 85 | 74,000,000 |
| UAN08A 4B M2C2S250H | 800A | 85 | 76,000,000 |
| UAN10A 4B M2C2S250J | 1000A | 85 | 78,000,000 |
| UAN12A 4B M2C2S250K | 1250A | 85 | 81,000,000 |
| UAN16A 4B M2C2S250L | 1600A | 85 | 85,000,000 |
| UAN20A 4B M2C2S250M | 2000A | 85 | 93,000,000 |
| UAN20B 4B M2C2S250M | 2000A | 100 | 103,000,000 |
| UAN25B 4B M2C2S250N | 2500A | 100 | 112,800,000 |
| UAN32B 4B M2C2S250P | 3200A | 100 | 140,000,000 |
| UAN40C 4B M2C2S250Q | 4000A | 100 | 205,000,000 |
| UAN50C 4B M2C2S250S | 5000A | 100 | 245,000,000 |

|  |  |
| --- | --- |
| **Phụ kiện ACB** | |
| **Bộ bảo vệ thấp áp (UANS V\_)** | |
| UVT Coil | 1,250,000 |
| UVT Time Delay Controller | 2,990,000 |

|  |  |
| --- | --- |
| **Phụ kiện ACB** | |
| **Khóa liên động -Mechanical Interlock (UANS \_)** | |
| Liên động 2 ACB ( cho A, B frame) | 18,000,000 |
| Liên động 3 ACB ( cho A, B frame) | 30,000,000 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Thông số** | | | | **Mã hàng** | **Đơn giá (VND)** |
| **HVG Fixed series (Only VCB Body)** | | | | | |
| 7.2kV | 8kA | 400A | Control Voltage:DC110V, 4NO+4NC | HVG1099AXA444A | 54,385,000 |
| 12.5kA | 630A | HVG1011AXA444A | 58,652,000 |
| 20kA | 630A | HVG1131BXA444A | 77,493,000 |
| 1250A | HVG1132BXA444A | 79,016,000 |
| 25kA | 630A | HVG1141BXA444A | 77,524,000 |
| 1250A | HVG1142BXA444A | 80,969,000 |
| **HVG Draw-Out series With E Cradle (without Shutter & Bushing)** | | | | | |
| 7.2kV | 8kA | 400A | Control Voltage:DC110V, 4NO+4NC | HVG1099AES444A | 64,451,000 |
| 12.5kA | 630A | HVG1011AES444A | 70,293,000 |
| 20kA | 630A | HVG1131BES444A | 89,064,000 |
| 1250A | HVG1132BES444A | 93,553,000 |
| 25kA | 630A | HVG1141BES444A | 92,553,000 |
| 1250A | HVG1142BES444A | 95,987,000 |
| **HVG Draw-Out series With F Cradle (with Shutter & Without Bushing)** | | | | | |
| 7.2kV | 8kA | 400A | Control Voltage:DC110V, 4NO+4NC | HVG1099AFS444A | 72,200,000 |
| 12.5kA | 630A | HVG1011AFS444A | 76,051,000 |
| 20kA | 630A | HVG1131BFS444A | 95,727,000 |
| 1250A | HVG1132BFS444A | 97,500,000 |
| 25kA | 630A | HVG1141BFS444A | 96,087,000 |
| 1250A | HVG1142BFS444A | 100,824,000 |
| **HVG Draw-Out series With G Cradle (with Shutter & Bushing)** | | | | | |
| 7.2kV | 8kA | 400A | Control Voltage:DC110V, 4NO+4NC | HVG1099AGS444A | 87,618,000 |
| 12.5kA | 630A | HVG1011AGS444A | 89,549,000 |
| 20kA | 630A | HVG1131BGS444A | 116,556,000 |
| 1250A | HVG1132BGS444A | 129,053,000 |
| 25kA | 630A | HVG1141BGS444A | 124,025,000 |
| 1250A | HVG1142BGS444A | 132,884,000 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **HVF Fixed series (Only VCB Body)** | | | | | |
| 36kV | 25kA | 1250A | Control Voltage:DC110V, 4NO+4NC | HVF7142IXA444C | 250,338,000 |
| 2000A | HVF7144IXA444C | 253,775,000 |
| 31.5kA | 1250A | HVF7052IXA444C | 280,006,000 |
| 2000A | HVF7054IXA444C | 313,273,000 |
| 3150A | HVF7057IXA444C | 348,379,000 |
| **HVF Draw-Out series With G Cradle (with Shutter & Bushing)** | | | | | |
| 36kV | 25kA | 1250A | Control Voltage:DC110V, 4NO+4NC | HVF7142IGS444C | 513,451,000 |
| 2000A | HVF7144IGS444C | 527,967,000 |
| 31.5kA | 1250A | HVF7052IGS444C | 591,598,000 |
| 2000A | HVF7054IGS444C | 681,500,000 |
| 3150A | HVF7057IGS444C | 894,715,000 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **HGV Fixed series (Only VCB Body)** | | | | |  |
| 7.2kV | 25kA | 630A | Control Voltage:AC/DC110V, 4NO+4NC | HGV1141CXA444C | 111,739,000 |
| 1250A | HGV1142CXA444C | 112,312,000 |
| 24/25.8kV | 25kA | 630A | HGV6141FXA444C | 124,919,000 |
| 1250A | HGV6142FXA444C | 125,492,000 |
| 2000A | HGV6144FXA444C | 148,413,000 |
| **HGV Draw-out series With E Cradle (without Shutter & Bushing)** | | | | |  |
| 7.2kV | 25kA | 630A | Control Voltage:AC/DC110V, 4NO+4NC | HGV1141CES444C | 137,525,000 |
| 1250A | HGV1142CES444C | 143,255,000 |
| 24/25.8kV | 25kA | 630A | HGV6141FES444C | 172,480,000 |
| 1250A | HGV6142FES444C | 173,339,000 |
| 2000A | HGV6144FES444C | 207,434,000 |
| **HGV Draw-out series with F Cradle (with Shutter & without Bushing)** | | | | |  |
| 7.2kV | 25kA | 630A | Control Voltage:AC/DC110V, 4NO+4NC | HGV1141CFS444C | 148,126,000 |
| 1250A | HGV1142CFS444C | 154,716,000 |
| 24/25.8kV | 25kA | 630A | HGV6141FFS444C | 179,585,000 |
| 1250A | HGV6142FFS444C | 183,252,000 |
| 2000A | HGV6144FFS444C | 252,015,000 |
| **HGV Draw-out series With G Cradle (with Shutter & Bushing)** | | | | |  |
| 7.2kV | 25kA | 630A | Control Voltage:AC/DC110V, 4NO+4NC | HGV1141FGS444C | 223,479,000 |
| 1250A | HGV1142FGS444C | 226,344,000 |
| 24/25.8kV | 25kA | 630A | HGV6141FGS444C | 226,344,000 |
| 1250A | HGV6142FGS444C | 237,804,000 |
| 2000A | HGV6144FGS444C | 269,951,000 |

|  |  |  |
| --- | --- | --- |
| **Mã hàng** | **Thông số** | **Đơn giá (VND)** |
| **Vacuum Contactor 3.6/7.2kV 200A, Continuously Energized, Fixed type** | | |
| UVC32CX1000000H | 3.6kV, 200A, without fuse holder, AC/DC 200-230V, 3NO+2NC | 30,136,000 |
| UVC62CX1000000H | 7.2kV, 200A, without fuse holder, AC/DC 200-230V, 3NO+2NC | 31,012,000 |
| UVC32CA1006000HCM | 3.6kV, 200A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, with FMD | 35,751,000 |
| UVC62CA1006000HCM | 7.2kV, 200A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, with FMD | 36,782,000 |
| **Vacuum Contactor 3.6/7.2kV 200A, Continuously Energized, Draw-out type** | | |
| UVC32CB1F10000H | 3.6kV, 200A, without fuse holder, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter) | 41,469,000 |
| UVC62CB1F10000H | 7.2kV, 200A, without fuse holder, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter) | 42,345,000 |
| UVC32CD1F16000CM | 3.6kV, 200A, with 192mm single fuse holder not including fuse,  AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter), with FMD | 48,991,000 |
| UVC62CD1F16000CM | 7.2kV, 200A, with 192mm single fuse holder not including fuse,  AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter), with FMD | 50,021,000 |
| HCA32CB4M10000 | 3.6kV, 200A, without fuse holder, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing) | 92,108,000 |
| HCA62CB4M10000 | 7.2kV, 200A, without fuse holder, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing) | 93,190,000 |
| HCA32CD4M16000AM | 3.6kV, 200A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing), with FMD | 100,917,000 |
| HCA62CD4M16000AM | 7.2kV, 200A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing), with FMD | 102,051,000 |
| HCA32CB4T10000 | 3.6kV, 200A, without fuse holder, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 142,747,000 |
| HCA62CB4T10000 | 7.2kV, 200A, without fuse holder, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 143,520,000 |
| **Vacuum Contactor 3.6/7.2kV 400A, Continuously Energized, Fixed type** | | |
| UVC34CX1000000H | 3.6kV, 400A, without fuse holder, AC/DC 200-230V, 3NO+2NC | 29,467,000 |
| UVC64CX1000000H | 7.2kV, 400A, without fuse holder, AC/DC 200-230V, 3NO+2NC | 30,342,000 |
| UVC34CA1006000HCM | 3.6kV, 400A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, with FMD | 36,782,000 |
| UVC64CA1006000HCM | 7.2kV, 400A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, with FMD | 37,915,000 |
| **Vacuum Contactor 3.6/7.2kV 400A, Continuously Energized, Draw-out type** | | |
| UVC34CB1F10000H | 3.6kV, 400A, without fuse holder, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter) | 42,706,000 |
| UVC64CB1F10000H | 7.2kV, 400A, without fuse holder, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter) | 43,633,000 |
| UVC34CD1F16000CM | 3.6kV, 400A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter), with FMD | 50,433,000 |
| UVC64CD1F16000CM | 7.2kV, 400A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter), with FMD | 51,566,000 |
| HCA34CB4M10000 | 3.6kV, 400A, without fuse holder, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing) | 94,890,000 |
| HCA64CB4M10000 | 7.2kV, 400A, without fuse holder, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing) | 95,972,000 |
| HCA34CD4M16000AM | 3.6kV, 400A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing), with FMD | 103,957,000 |
| HCA64CD4M16000AM | 7.2kV, 400A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing), with FMD | 105,141,000 |
| HCA34CB4T10000 | 3.6kV, 400A, without fuse holder, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 147,023,000 |
| HCA64CB4T10000 | 7.2kV, 400A, without fuse holder, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 147,847,000 |
| HCA34CD4T16000AM | 3.6kV, 400A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch), with FMD | 159,500,000 |
| HCA64CD4T16000AM | 7.2kV, 400A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch), with FMD | 161,500,000 |

|  |  |  |
| --- | --- | --- |
| **Mã hàng** | **Thông số** | **Đơn giá (VNĐ)** |
| **Vacuum Contactor 3.6/7.2kV 200A, Latched, Fixed type** | | |
| UVC32LX1000000H | 3.6kV, 200A, without fuse holder, AC/DC 200-230V, 3NO+2NC | 31,012,000 |
| UVC62LX1000000H | 7.2kV, 200A, without fuse holder, AC/DC 200-230V, 3NO+2NC | 32,763,000 |
| UVC32LA1006000HCM | 3.6kV, 200A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, with FMD | 37,554,000 |
| UVC62LA1006000HCM | 7.2kV, 200A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, with FMD | 38,636,000 |
| **Vacuum Contactor 3.6/7.2kV 200A, Latched, Draw-out type** | | |
| UVC32LB1F10000H | 3.6kV, 200A, without fuse holder, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter) | 43,581,000 |
| UVC62LB1F10000H | 7.2kV, 200A, without fuse holder, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter) | 44,509,000 |
| UVC32LD1F16000CM | 3.6kV, 200A, with 192mm single fuse holder not including fuse,  AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter), with FMD | 51,463,000 |
| UVC62LD1F16000CM | 7.2kV, 200A, with 192mm single fuse holder not including fuse,  AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter), with FMD | 52,545,000 |
| HCA32LB4M10000 | 3.6kV, 200A, without fuse holder, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing) | 96,693,000 |
| HCA62LB4M10000 | 7.2kV, 200A, without fuse holder, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing) | 97,878,000 |
| HCA32LD4M16000AM | 3.6kV, 200A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing), with FMD | 105,966,000 |
| HCA62LD4M16000AM | 7.2kV, 200A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing), with FMD | 107,202,000 |
| HCA32LB4T10000 | 3.6kV, 200A, without fuse holder, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 149,908,000 |
| HCA62LB4T10000 | 7.2kV, 200A, without fuse holder, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 150,732,000 |
| HCA32LD4T16000AM | 3.6kV, 200A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch), with FMD | 163,500,000 |
| HCA62LD4T16000AM | 7.2kV, 200A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch), with FMD | 165,000,000 |
| **Vacuum Contactor 3.6/7.2kV 400A, Latched, Fixed type** | | |
| UVC34LX1000000H | 3.6kV, 400A, without fuse holder, AC/DC 200-230V, 3NO+2NC | 30,909,000 |
| UVC64LX1000000H | 7.2kV, 400A, without fuse holder, AC/DC 200-230V, 3NO+2NC | 31,836,000 |
| UVC34LA1006000HCM | 3.6kV, 400A,with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, with FMD | 38,636,000 |
| UVC64LA1006000HCM | 7.2kV, 400A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, with FMD | 39,821,000 |
| **Vacuum Contactor 3.6/7.2kV 400A, Latched, Draw-out type** | | |
| UVC34LB1F10000H | 3.6kV, 400A, without fuse holder, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter) | 44,818,000 |
| UVC64LB1F10000H | 7.2kV, 400A, without fuse holder, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter) | 45,797,000 |
| UVC34LD1F16000CM | 3.6kV, 400A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter), with FMD | 52,957,000 |
| UVC64LD1F16000CM | 7.2kV, 400A, with 192mm single fuse holder not including fuse, AC/DC 200-230V, 3NO+2NC, With F Cradle (Insulation shutter), with FMD | 54,090,000 |
| HCA34LB4M10000 | 3.6kV, 400A, without fuse holder, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing) | 99,629,000 |
| HCA64LB4M10000 | 7.2kV, 400A, without fuse holder, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing) | 100,814,000 |
| HCA34LD4M16000AM | 3.6kV, 400A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing), with FMD | 109,160,000 |
| HCA64LD4M16000AM | 7.2kV, 400A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With M Cradle (Metal shutter and bushing), with FMD | 110,345,000 |
| HCA34LB4T10000 | 3.6kV, 400A, without fuse holder, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 154,441,000 |
| HCA64LB4T10000 | 7.2kV, 400A, without fuse holder, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 155,265,000 |
| HCA34LD4T16000AM | 3.6kV, 400A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 168,000,000 |
| HCA64LD4T16000AM | 7.2kV, 400A, with 192mm single fuse holder not including fuse, AC220V, 2NO+2NC, With T Cradle (Metal shutter, Bushing, & Earthing switch) | 169,500,000 |